# SECTION 106

**CONTROL OF MATERIAL**

Standard Modification

**106-1.02 MATERIAL SOURCES.**

*ADD the following new Item:*

5. c. Extraction of material below or within four feet of the seasonal high water table requires a permit under MSB Code Chapter 17.30.

MSB 082719